**Linear Quadratic Integral Differential Game applied to the Real-time Control of a Quadrotor Experimental setup**

Hadi Nobahari\*, Ali Baniasad, Reza Pordal and Alireza Sharifi

Sharif University of Technology, Zip Code 1458889694, Tehran, Iran

nobahari@sharif.edu, [alireza\_sharifi@ae.sharif.edu](mailto:alireza_sharifi@ae.sharif.edu), ali.baniasad@ae.sharif.edu

**Abstract.**

The accurate attitude control of a quadrotor is necessary, especially when facing disturbance. Moreover, all the flight states of the quadrotor are not measured in practice. In this study, a linear quadratic Gaussian with integral action based on the differential game theory is implemented on the quadrotor experimental setup. A continuous state-space model of the setup is derived using the linearization of nonlinear equations of motion, and its parameters are identified with the experimental results. Then, the variables of the quadrotor setup are estimated based on an extended Kalman filter to compensate in the controller structure. Next, the attitude control commands of the quadrotor are derived based on two players; one finds the best attitude control command, and the other creates the disturbance by mini-maximizing a quadratic criterion, defined as the sum of outputs plus the weighted control effort and disturbance. The performance of the proposed structure is investigated in level flight and compared to the linear quadratic regulator controller. Results demonstrate that the proposed approach has an excellent performance in dissipating the disturbances.

**Keywords:** Linear Quadratic Gaussian, Differential Game, Quadrotor, State Estimation, 3DoF Experimental setup, Optimal Control, Robust Control.

\*Corresponding Author.

1. Introduction

A quadrotor is a type of helicopter with four rotors that plays a significant role in today's society (Fathoni, 2021), including research, military, imaging, recreation, and agriculture. The performance of the quadrotor relies on the control system, including attitude, altitude, and position subsystems. In the attitude control of the quadrotor, it is vital to maintain the attitude outputs at the desired level using control commands such as the rotational speed of the rotors (Sharifi, 2019), when the disturbances occur suddenly. Therefore, much research is being conducted on the automatic control of the attitudes' quadrotor in facing the disturbance.

In (H. Bolandi, 2013) (Abdul Salam, 2019), a Proportional Integral Derivative (PID) controller is used to regulate the quadrotor attitude. However, the control objectives have not been effectively achieved with this controller when the disturbance occurs. To solve this problem the model-based approaches (Bouzid, 2020) (Wang, 2020) are utilized for controller design. These controllers work based on information from the quadrotor's attitude model and disturbance to produce the best control command.

Various model-based controllers can be found within the literature, the most well-known of which are intelligent control, the nonlinear control, robust control, and optimal control to reduce the disturbance effect in the attitude control and provide a faster control algorithm in facing the modeling error. In the intelligent controller category, the artificial intelligence computing approaches like fuzzy logic (K. Liu, 2022) iterative learning (L. V. Nguyen, 2021) machine learning (C. Nicol, 2008), reinforcement learning (C.-H. Pi, 2021), and evolutionary computation (P. Ghiglino, 2013) have been utilized to regulate the quadrotor's attitude.

Nonlinear control methods such as Feedback Linearization (FBL) (A. Aboudonia, 2016), Sliding Mode Control (SMC) (Chen, 2014) and Synergetic Control (Chara, 2022) have been applied to control the roll, pitch, and yaw angles of the quadrotor. Moreover, robust control strategies such as  (Azar, 2020) (El-Badawy) and  (Dean, 2017) have been implemented to stabilize the quadrotor attitudes based on the worst-case scenario and large uncertainty ranges. In the optimal controller category, a Linear Quadratic Regulator (LQR) (Z. Shulong, 2013) and Linear Quadratic Gaussian (LQG) (E. Barzanooni, 2015) have been implemented on the quadrotor based on the minimization of a quadratic criterion, including regulation performance and control effort to provide optimally controlled feedback gains.


Linear Quadratic Regulator Differential Game (LQR-DG) control approach (Engwerda J. C., 2006), (Engwerda J. , 2022) is a class of optimal and robust controller methods that controls the outputs of a system based on its linear model and mini-maximization of a cost function. This approach has been utilized to stabilize and control various nonlinear and complex systems such as a ship controller (Zwierzewicz, 2014) (Li, 2011). Moreover, in the LQR-DG control method, the control commands are analytically generated based on a pursuit-evasion of two players, one tracks the best control command, and the other creates the disturbance. This is one of the distinctive features of the LQR-DG controller and an important difference from other optimal control methods.

In this study, a LQG controller method based on the differential game theory, with an integral action called Linear Quadratic Integral Gaussian Differential Game (LQIG-DG) controller, is proposed to generate the most efficient control command for an experimental setup of the quadrotor when facing the disturbance. Since the LQIG-DG is affected by an accurate model of the system, first, the dynamic of the three-degree-of-freedom setup of the quadrotor is modeled. Then, the linear state-space form the quadrotor model is extracted using the linearization of the nonlinear equations of motion to utilize in the proposed control problem. Moreover, the model's parameters are identified and verified against the experimental values. Next, the flight states of the quadrotor setup are estimated based on an Extended Kalman Filter (EKF) (Kunwu Zhang, 2016) (Azid, 2021) and then compensated using the LQIG-DG controller architecture. Finally, the LQIG-DG technique is applied to the experimental setup of the quadrotor to reduce the effect of disturbance. The performance of the suggested controller is examined when the disturbance occurs. The results show the successful performance of the LQIR-DG scheme in reducing the disturbance.

In the remainder of this study, the problem is defined in section ‎2. In sections ‎3, the dynamics model for the experimental setup of the quadrotor and the estimation problem are derived in details, respectively. In section , the LQIR-DG architecture is denoted. Finally, in sections ‎5 and ‎6, numerical results and conclusion are provided, respectively.

1. Problem Statement

Here, a nonlinear dynamic is presented for the setup of the quadrotor, as illustrated in Fig. 1. The quadrotor is free to rotate about its roll, pitch, and yaw axes. The Euler angles and angular velocities along three orthogonal axes are measured using the Attitude and Heading Reference Systems (AHRS). These noisy measurements are utilizes in the LQIR-DG for control of the Euler angles. The block diagram of the controller structure is illustrated in Fig. 2.




**Fig. 1.** 3DoF setup of the quadrotor.

Microcontroller



3DOF setup of the quadrotor



Low Cost IMU

Attitude Command





Roll Loop Controller

Pitch Loop Controller

Yaw Loop Controller Control

*u*roll

*u*pitch

*u*yaw

Microcontroller: LQIR-DG

**Fig. 2.** Block diagram of the LQIG-DG controller structure.

1. Modeling of the Quadrotor Setup

Here, the model of the three-degree-of-freedom setup of the quadrotor is presented in details. For this purpose, first, the configuration of the quadrotor is denoted. Then, the nonlinear model of the attitude dynamics is derived to denote the state-space form. In the next step, the nonlinear model is linearized to utilize in the control purposes. Finally, the model parameters of the 3DOF experimental setup are identified based on the experimental data.

* 1. Configuration of the Quadrotor

Fig. 3 denotes the quadrotor schematic. Each rotor has an angular velocity, , rotating about the  axis in the body coordinate system. Rotors 1 and 3 rotate counterclockwise, while rotors 2 and 4 rotate clockwise, to cancel yawing moment.

M4

xB

yB

zB







ZI

XI

xB

yB









M1

M3

M2

dcg

YI

**Fig. 3.** Configuration of the quadrotor

* 1. Dynamic Model

The quadrotor kinetic model, derived using the Newton-Euler method, is stated as (Bouabdallah, 2007), (Siegwart, 2007)

|  |  |
| --- | --- |
|  | (1) |
|  | (2) |
|  | (3) |

where  are the angular velocities. , , and  are the disturbances, generated in , . and , respectively. Moreover, , , and  are the principal moment of inertia and  is a rotor inertia about its axis. The relation between the angular body rates and the Euler angles rates are obtained as

|  |  |
| --- | --- |
|  | (4) |
|  | (5) |
|  | (6) |

where  are roll, pitch, and yaw angles. Moreover, , called the overall residual rotor angular velocity, is computed as

|  |  |
| --- | --- |
|  | (7) |

* 1. Control Commands

The control inputs , , and  are roll, pitch, and yaw moments, obtained from the rotors, defined as

|  |  |
| --- | --- |
|  | (8) |
|  | (9) |
|  | (10) |

Also, d and b are, respectively, drag and thrust coefficients.  is the distance of rotors from the gravity center . Hence, the angular velocity commands are obtained as

|  |  |
| --- | --- |
|  | (11) |
|  | (12) |
|  | (13) |
|  | (14) |

where  is the nominal of the rotor angular velocities.

* 1. State-Space Form

Here, the state-space model is presented for the control purposes. By defining , , , , , and ; the model of in state-space form are denoted as

|  |  |
| --- | --- |
|  | (15) |
|  | (16) |
|  | (17) |
|  | (18) |
|  | (19) |
|  | (20) |

Moreover,  (*i*=1,…,8) is defined as

|  |  |
| --- | --- |
|  | (21) |

The measurement model is written as

|  |  |
| --- | --- |
|  | (21) |

* 1. Linear Model

The continuous-time linear model is utilized to drive the control commands on the quadrotor. The linear state-space model is denoted as

|  |  |
| --- | --- |
|  | (22) |

where , , and  are the system, input and disturbance matrices, respectively. Moreover,  is the disturbance. The measurements equation is stated as

|  |  |
| --- | --- |
|  | (23) |

According to Eqs.(15)-(20) the linear dynamic model around the equilibrium points  of. the quadrotor setup is denoted as

|  |  |
| --- | --- |
|  | (24) |

where , , and . Moreover, the state and input matrices are presented as

|  |  |
| --- | --- |
|  | (25) |
|  | (26) |

* 1. Identification of the Setup Parameters

In this section, the optimization technique based on the Nonlinear Least Squares (NLS) method is utilized to estimate the model parameters () for the 3DOF experimental setup from experimental data. Here, the NLS algorithm, that is based on the trust-region reflective least squares (TRRLS) method, finds iteratively the values of the model parameters based on the minimization of the cost function, so that the input/output signals provided by the simulation model are very similar to the experimental ones. Therefore, the least squares problem consists in finding a vector  that minimizes a sum of squares function [?], as follows:

|  |  |
| --- | --- |
|  | (25) |

where  and  are the simulated and experimental outputs, when the same input signals are applied ones. Moreover, a vector  has upper and lower bound constraints, ub and lb, respectively, with lb . The structure of the proposed identification approach is illustrated in Figure 1.

Figure 5. Structure of TRRLS identification approach.

1. Formulation of the Controller Design

In the LQIR-DG controller structure, an integral action is added to the LQR-DG controller to cancel the steady-state errors for reference tracking. For this purpose, first, the augmented state space of the linear quadrotor model is defined to utilize in the controller architecture. Then, the LQR-DG controller design procedure is presented to produce the best control commands for the experimental setup of the quadrotor.

* 1. Augmented State Space Formulation

To add the integral action to the controller structure, the augmented states are defined as follows:

|  |  |
| --- | --- |
|  | (27) |

where  = roll, pitch, and yaw.

Then, the quadrotor dynamics model, denoted by Eq.(**22**), is denoted in the augmented state-space model as

|  |  |
| --- | --- |
|  | (28) |

where matrices  and  are defined as follows:

|  |  |
| --- | --- |
|  | (29) |
|  | (30) |

In the above equation  denotes the identity matrix.

* 1. LQIR-DG Controller Method

The LQIR-DG controller is an optimal and robust method based on the differential game theory. This controller consists of two essential players: one finds the best control command, and the other creates the worst disturbance.

For this purpose, the first player tries to minimize a cost function; while the second player is assumed to maximize it. Therefore, the quadratic cost function equation is denoted using min-max operators as follows:



|  |  |
| --- | --- |
|  | (31) |

where  and  are symmetric nonnegative definite matrices and  is a symmetric positive definite matrix. Moreover,  is the final time. To solve this problem, connections between the general optimal problem and the LQIR problem are considered (Engwerda J. C., 2006) and consequently the optimum control effort is computed for the each control loop as follows:

|  |  |
| --- | --- |
|  | (32) |
|  | (33) |

where  and  are a time varying gain, given by

|  |  |
| --- | --- |
|  | (34) |
|  | (35) |

where  and  satisfy

|  |  |
| --- | --- |
|  | (36) |
|  | (37) |
|  |  |

where  and .

In this study, the steady-state values of the above equations  are utilized to generate a feedback control law.

1. Result and Discussion

Here, the results of the LQIR-DG controller method are devoted to the control loops of the roll, pitch, and yaw of the experimental setup of the quadrotor. First, the controller parameters are tuned using the results of numerical simulations. Moreover, the performance of the LQIR-DG controller is compared to an LQR control strategy. The quadrotor parameters are shown in **Table 1**. Moreover, the parameters of LQIR-DG controller weight are denoted in **Table 2**.

**Table 1.** The Parameter of the Quadrotor.

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Value |
|  |  | 0.02839 |
|  |  | 0.03066 |
|  |  | 0.0439 |
|  |  |  |
| b |  |  |
| d |  |  |
|  | rpm | 3000 |
|  |  | 0.2 |

**Table 2.** The Parameters of the LQIR-DG Controller.

|  |  |  |
| --- | --- | --- |
| Control Loop | Weight | Value |
| Roll |  | diag([7.91,0.01,631.85, 214.28]) |
| Pitch |  | diag([9853.09, 0.12, 0.01, 873.93]) |
| Yaw |  | diag([1.81e-4, 4.5e-4, 3e-6, 1.7e-5]) |
| - |  | 1 |
| - |  | 1.2577 |

* 1. Identification of the 3DoF experimental setup model

As denoted in section ?, the parameters of the quadrotor setup are  (*i*=1,…,8) that need to be identified based on the NRS algorithm. The NLS-TRRLS algorithm is performed in the Matlab R2022a®. In order to increase accuracy identification of parameters, three scenarios, according to Table 3, are considered and performed. When the stopping condition of the NLS algorithm is reached, the best values of the quadrotor parameters are computed, shown in Table 4. Moreover, the intelligent movement of the parameters during the optimization process for finding the true values is shown in Figure 9.

In the first scenario, according to the Figure ?, the quadrotor is able to rotate about only one axis (roll, pitch or yaw axes) to identify ,  and  parameters. In the second scenario, Figure ? shows  and  parameters are estimated based on the experimental setup, that is free to rotate around its roll and pitch axes. Finally, in the last scenario, according to the Figure ?, ,  and  parameters of the UAV model are identified by rotate the quadrotor setup around three axis. These results illustrate that the outputs of the simulation results for the quadrotor model are consistent with reality.

Tabel :Scenarios for identification of quadrotor model.

|  |  |  |  |
| --- | --- | --- | --- |
| Scenario | Description | Initial Conditions | angular velocity Commands |
| I | Roll free | 10 | 10 |
| Pitch free |  |  |
| Yaw free |  |  |
| Ii | Roll & Pitch Free | 10 | 5 |
| Iii | Roll, Pitch and Yaw free | 20 | 10 |

**Table 4.** True values of the quadrotor parameters.

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Value | Parameter | Value |
|  | 69 |  |  |
|  | 37 |  |  |
|  | 7.96e15 |  |  |
|  | 1 |  |  |

|  |  |
| --- | --- |
|  |  |
| (a) | |
|  |  |
| (b) | |
|  |  |
|  | |

Figure . Identification process results when the quadrotor rotates about only one axis: (a) Identification of  in free roll. (b) Identification of  in free pitch. (c) Identification of  in free yaw.

|  |  |
| --- | --- |
|  |  |
| (a) | |
|  |  |
| (b) | |

Figure . Identification process results when the quadrotor rotates about its roll and pitch axes: (a) Comparison of Simulation and experimental results. (b) Identification of  and .

|  |  |  |
| --- | --- | --- |
|  |  |  |
| (a) | | |
|  |  |  |
| (b) | | |

Figure . Identification process results when the quadrotor rotates about its roll, pitch and yaw axes: (a) Comparison of Simulation and experimental results. (b) Identification of ,  and  parameters.





* 1. Performance of the LQIR-DG Controller

Here, the performance of the LQIR-DG controller is evaluated. The desired and actual outputs, including the roll, pitch, and yaw angles, are compared in **Fig. 4**. The desired scenario of the simulator is considered as a level flight. These figures show that the attitude outputs of the quadrotor converge to the desired values in less than three seconds. Moreover, **Fig. 5** show the angular velocity command of the quadrotor, respectively. These results illustrate that the LQIR-DG approach appropriately controls the attitude of the experimental setup of the quadrotor.

**Fig. 8** illustrates the performance of the LQIR-DG controller in the coupling mode of the roll and pitch channels to track the desired angle as a square wave with a frequency of 0.02 Hz and an amplitude of 20 degrees.

|  |  |  |
| --- | --- | --- |
|  |  |  |
| (a) | (b) | (c) |

**Fig. 4.** Performance of the LQIR-DG controller (a) roll angle (b) pitch angle (c) yaw angle



**Fig. 5.** Time history of angular velocity commands

|  |  |
| --- | --- |
|  |  |
| (a) | (b) |

**Fig. 6.** LQIR-DDG controller performance in order to track the desired angles in the two-degree-of-freedom coupling mode a) Comparison of the roll angle with the desired value b) Comparison of the pitch angle with the desired

* 1. Investigating the possibility of disturbance rejection


This section investigates the possible rejection of input disturbances by the LQIR-DG controller in regulation. For this purpose, a disturbance with an amplitude of 0.5 N is added to the input from 26 to 36 seconds. As shown in Fig. 7, the LQIR-DG controller performs well in coupling the roll and screw channels to remove the input disturbance. In Fig. 7 (a), the performance of this controller is checked by comparing the desired roll angle with the actual roll angle. Also, Fig. 7 (b) compares the desired turn angle with the actual pitch angle of the 3DoF experimental setup in removing the input disturbance. The results indicate the proper performance of the controller in removing the input disturbance.



|  |  |
| --- | --- |
|  |  |
|  |  |

**Fig. 7.** The performance of the LQIR-DG controller in the presence of the input disturbance in the two-degree-of-freedom coupling mode a) Comparison of the desired roll angle with the actual value b) Comparison of the desired pitch angle with the actual value.

* 1. Investigating the impact of uncertainty in modeling

This section examines the performance of the LQIR-DG controller designed by considering the uncertainty in 3DoF experimental setup modeling. The performance of the sliding mode controller in the coupling mode of the roll, pitch, and yaw channels is checked by considering the uncertainty in the 3DoF experimental setup modeling in figure 17. For this purpose, 50 grams is added to the roll axis and 100 grams to the pitch axis. In figure 17 (a), the performance of this controller is checked by comparing the desired roll angle with the actual roll angle; In figure 17 (b), the performance of this controller is checked by comparing the desired pitch angle to the actual pitch angle. The implementation results indicate the proper efficiency of the LQIR-DG controller in pursuit of the desired value, taking into account the uncertainty in the values of the moments of inertia around each axis of the body coordinate system.







**Fig. 7.** The performance of the LQIR-DG controller by adding weight to each of the roll and pitch axes in the two-degree-of-freedom coupling mode (a) Comparison of the roll angle with the actual value (b) Comparison of the pitch angle with the actual value

* 1. Comparison with LQR, LQIR, and PID

Here, the LQIR-DG controller performance is compared with famous control strategies such as the LQR controller method. Figure18 compares the quadrotor’s desired and actual pitch angle in the presence of these controllers. This result indicates that the LQIR-DG controller can provide high tracking performance, such as good transient response and high rapid convergence relative to the LQR controller for pitch angle control of the quadrotor setup.



**Fig. 8.** The performance of the LQIR-DG controller by adding weight to each of the roll and pitch axes in the three-degree-of-freedom coupling mode (a) Comparison of the roll angle with the actual value (b) Comparison of the pitch angle with the actual value (c) Comparison of the yaw angle with the actual value

Figure 19: Comparison of the LQIR-DG to the PID quadratic cost function

Figure 19: Comparison of the LQIR-DG to the PID quadratic cost function

Figure 19: Comparison of the LQIR-DG to the PID quadratic cost function

Figure 19: Comparison of the LQIR-DG to the PID quadratic cost function




Figure 19: Comparison of the LQIR-DG to the PID quadratic cost function

1. Conclusion

In this study, a linear quadratic with integral action based on the differential game theory, called LQIR-DG, was implemented for level attitude control in an experimental setup of a quadrotor. To implement the proposed controller structure, first, an accurate model of the quadrotor was linearized in the state-space form, and then the model parameters were estimated. Next, two players were considered for each of the quadrotor's roll, pitch, and yaw channels. The first player found the best control command for each channel of the setup of a quadrotor based on the mini-maximization of a quadratic criterion; when the second player produced the worst disturbances. Finally, the performance of the proposed controller was investigated in level flight and compared to the LQR controller. The implementation results verify the successful performance of the LQIR-DG method in the level flight of the attitude control for the actual plant.

# Bibliography

H. Bolandi, M. R. (2013). Attitude Control of a Quadrotor with Optimized PID Controller. *Intelligent Control and Automation, 4*, 335-342.

Boosting a Reference Model-Based Controller Using Active Disturbance Rejection Principle for 3D Trajectory Tracking of Quadrotors: Experimental Validation2020*Journal of Intelligent and Robotic Systems*597–614

Adaptive Fuzzy Finite-time Attitude Controller Design for Quadrotor UAV with External Disturbances and Uncertain Dynamics2022*8th International Conference on Control, Automation and Robotics (ICCAR)*363-368

Iterative Learning Sliding Mode Control for UAV Trajectory Tracking2021*Electronics10*

Robust neural network control of a quadrotor helicopter2008*Canadian Conference on Electrical and Computer Engineering*

Robust Quadrotor Control through Reinforcement Learning with Disturbance Compensation2021*Applied Sciences11*

Online PID Self-Tuning using an Evolutionary Swarm Algorithm with Experimental Quadrotor Flight Results2013*AIAA Guidance Navigation, and Control (GNC) Conference*

Disturbance observer-based feedback linearization control of an unmanned quadrotor helicopter2016*Proceedings of the Institution of Mechanical Engineers, Part I: Journal of Systems and Control Engineering230*877–891

Sliding mode attitude control for a quadrotor micro unmanned aircraft vehicle using disturbance observer2014*IEEE Chinese Guidance, Navigation and Control Conference*568-573

A new feedback linearization LQR control for attitude of quadrotor2013*13th International Conference on Control Automation Robotics and Vision (ICARCV)*1593-1597

Attitude flight control system design of UAV using LQG multivariable control with noise and disturbance2015*3rd RSI International Conference on Robotics and Mechatronics (ICROM)*188-193

Linear Quadratic Games: An Overview2006

On the ship course-keeping control system design by using robust and adaptive control2014*9th International Conference on Methods and Models in Automation and Robotics (MMAR)*189-194

Min-Max Robust Control in LQ-Differential Games2022*Dynamic Games and Applications*

Design and Control of Quadrotors with Application to Autonomous Flying2007*(Ph.D. thesis), University of Pennsylvania, Philadelphia*

Full control of a quadrotor2007*IEEE/RSJ International Conference on Intelligent Robots and Systems*153-158

Backstepping H-Infinity Control of Unmanned Aerial Vehicles with Time Varying Disturbances2020

EKF-based LQR tracking control of a quadrotor helicopter subject to uncertainties2016

Development of Multi-Quadrotor Simulator Based on Real-Time Hypervisor Systems2021*Drones5*

A hybridization of extended Kalman filter and Ant Colony Optimization for state estimation of nonlinear systems2019*Applied Soft Computing74*411-423

Active Disturbance Rejection Control of Quadrotor UAV based on Whale Optimization Algorithm2022*2022 IEEE International Conference on Mechatronics and Automation (ICMA)*351-356

Nonlinear PID controller design for a 6-DOF UAV quadrotor system2019*Engineering Science and Technology, an International Journal}*

Active disturbance rejection control for a quadrotor UAV2020*2020 IEEE 9th Data Driven Control and Learning Systems Conference (DDCLS)*1-5

A robust synergetic controller for Quadrotor obstacle avoidance using Bézier curve versus B-spline trajectory generation2022*Intelligent Service Robotics*

Robust H-infinity Control for a Quadrotor UAV*AIAA SCITECH 2022 Forum*

Robust Gust Rejection on a Micro-air Vehicle Using Bio-inspired Sensing2017*Mechatronics and Robotics Engineering for Advanced and Intelligent Manufacturing*351-362

Towards a Theory of stochastic adaptive differential games2011*2011 50th IEEE Conference on Decision and Control and European Control Conference*5041-5046

Robust Motion Control of Nonlinear Quadrotor Model With Wind Disturbance Observer2021*IEEE Access*149164-149175